<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<packages>
<package name="DBV">
</package>
<package name="P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="P-LCC-4-3">
<description>&lt;b&gt;Hyper TOPLED® &lt;/b&gt;&lt;p&gt;

The pin numbering on this package is exactly opposite of the CREE LED. This one matches the Chinese knock off brand.

&lt;/p&gt;</description>
</package>
<package name="SM-R6">
<description>SMD TOROIDAL CORE &lt;B&gt;TRANSFORMER&lt;/B&gt;&lt;p&gt;
10.8 x 8.8 x 5.5 mm</description>
</package>
<package name="EMC13">
</package>
<package name="B82464">
</package>
<package name="TO220AB">
<description>&lt;B&gt;TO220 AB&lt;/B&gt;&lt;p&gt;
3-lead molded horzintal</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="1X10">
</package>
<package name="1X10-2MM">
</package>
<package name="1X10-2MM-SMD">
</package>
<package name="1X10_LOCK">
</package>
<package name="1X10_LOCK_LONGPADS">
</package>
<package name="1X10-2MM-MALE-SMD">
</package>
<package name="MSOP10">
<description>&lt;b&gt;10 Lead Platic MSOP&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com .. LT1996</description>
</package>
<package name="CURRENTPLANK_STCS2A_POWER-SO10">
<description>&lt;b&gt;Power SO-10&lt;/b&gt;&lt;p&gt;
http://eu.st.com/stonline/ 3732.pdf and 5691.pdf</description>
</package>
<package name="CREE_XLAMP">
<description>&lt;b&gt;Cree® XLamp® XP-E LEDs&lt;/b&gt;&lt;p&gt;
Source: www.cree.com/xlamp .. XLampXP-E.pdf</description>
</package>
<package name="RE200B">
</package>
<package name="SPARK_LOGO">
</package>
<package name="SPARK_LOGO2">
</package>
<package name="SPARK_CORE">
</package>
<package name="SPARK_LOGO_PLUS_PLANE">
</package>
<package name="SRD-5VDC-SL-C">
</package>
<package name="RELAY-G5Q">
</package>
<package name="RELAY-T9A">
<description>Big relay. 220V/30A. SparkFun SKU: COM-00101</description>
</package>
<package name="RELAY-T9A-2">
</package>
<package name="RELAY-JZC">
</package>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S">
<description>&lt;b&gt;USB Series A Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-MB-H">
<description>&lt;b&gt;USB Series Mini-B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-SMT">
<description>USB Series B Surface Mounted</description>
</package>
<package name="USB-MINIB-OLD">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="S4B-PH">
</package>
<package name="USB-MINIB">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-PCB">
</package>
<package name="USB-B-PTH-VERTICAL">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="USB-A-S-NOSILK">
</package>
<package name="USB-A-S-NOSILK-FEMALE">
</package>
<package name="USB-MINIB-NOSTOP">
</package>
<package name="USB-A-S-SILK-FEMALE">
</package>
<package name="USB-MICROB">
<description>Micro USB Package</description>
</package>
<package name="USB-A-SMT-MALE">
</package>
<package name="USB-MICROB-ALIGN">
</package>
<package name="FC135">
<description>&lt;B&gt;Abracon ABS07 32.768 kHz crystal&lt;/B&gt;
&lt;P&gt;3.2 x 1.5 x 0.9mm</description>
</package>
<package name="HC49UP">
<description>CRYSTAL SMD</description>
</package>
<package name="TC38">
<description>Crystal TC38</description>
</package>
<package name="HC49U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TC38-SMD">
</package>
<package name="OSC3.2X.2.5">
</package>
<package name="SOIC127P790X216-8N">
</package>
<package name="WSON-8-PAD">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="IPEX-20279-001E">
</package>
<package name="AT8010">
</package>
<package name="EIA3216">
</package>
<package name="PC0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
<package name="USB-MICROB-SMT-DIP">
</package>
<package name="USB-MICROB-SLOT-HOLE">
</package>
<package name="1X12-SMALL-PADS">
</package>
<package name="1X12_LOCK">
</package>
<package name="1X12_LOCK_LONGPADS">
</package>
<package name="1X12_MACHINE-PIN-HEADER_LOCK.004">
</package>
<package name="1X12_LONGPADS">
</package>
<package name="1X12_HOLES_ONLY">
</package>
<package name="DIODE-DO-220AA(SMP)">
</package>
<package name="SPARK_CORE_STACKABLE">
</package>
<package name="POWER_JACK_SMD">
</package>
<package name="POWER_JACK_SLOT">
</package>
<package name="POWER_JACK_PTH">
</package>
<package name="POWER_JACK_COMBO">
</package>
<package name="POWER_JACK_PTH_LOCK">
</package>
<package name="OSHW-LOGO-S">
</package>
<package name="OSHW-LOGO-M">
</package>
<package name="OSHW-LOGO-L">
</package>
<package name="SOT-553">
</package>
<package name="SOT-953">
</package>
<package name="JS1-5V-F">
<description>RELAY GEN PURPOSE SPST 10A 5V</description>
</package>
<package name="G5LE-14-DC5">
</package>
<package name="INDUCTOR-1206">
</package>
<package name="0603">
</package>
<package name="CR54">
</package>
<package name="CDRH125">
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="B82462G">
</package>
<package name="CR75">
</package>
<package name="1210">
</package>
<package name="1007">
<description>1007 (2518 metric) package</description>
</package>
<package name="COOPER_UP4B">
</package>
<package name="CDRH3D28">
</package>
<package name="0805">
</package>
<package name="CR75_V2">
</package>
<package name="CDRH2D09">
<description>1.3x1.3mm 1.7mm between. Fits Sumida CDRH2D09, CDRH2D18 inductor</description>
</package>
<package name="NPI75C">
</package>
<package name="SRU5028">
</package>
<package name="SRU1038">
</package>
<package name="CR54-KIT">
</package>
<package name="DR1030">
<description>For Coiltronics/Cooper DR1030 series inductors</description>
</package>
<package name="VLF4012A">
</package>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="RLB0912">
</package>
<package name="SRN6045">
</package>
<package name="INDUCTOR-NR3015">
</package>
<package name="INDUCTOR-VLS-E">
</package>
<package name="USB-MICROB-MALE-SANDWICH">
</package>
<package name="SO08">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AA</description>
</package>
<package name="INDUCTOR-SDR1005-470KL">
</package>
<package name="SPARK_LOGO_TSTOP">
</package>
<package name="DHT22">
</package>
<package name="TGS2602">
</package>
<package name="MICS5525">
</package>
<package name="MQ_SENSOR_SOCKET">
</package>
<package name="TESTPAD-PTR">
</package>
<package name="SC70">
</package>
<package name="SC70-6">
<description>&lt;b&gt;6-Lead Thin Shrink Small Outline Transistor Package SC70&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4853-1_4853-2_4853-3.pdf</description>
</package>
<package name="WM-N-BM-09">
</package>
<package name="ML20">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
<package name="ML20L">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
<package name="3M_20">
<description>&lt;b&gt;3M&lt;/b&gt;</description>
</package>
<package name="3M_20L">
<description>&lt;b&gt;3M&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="UCC28700">
<pin name="CBC"/>
<pin name="VDD"/>
<pin name="DRV"/>
<pin name="VS"/>
<pin name="GND"/>
<pin name="CS"/>
</symbol>
<symbol name="RGBLED">
</symbol>
<symbol name="LED-RGB">
<pin name="CGREEN" direction="pas"/>
<pin name="CBLUE" direction="pas"/>
<pin name="CRED" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="SMR6-3">
<description>Wurth EMC13</description>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="1"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="TRIAC">
</symbol>
<symbol name="TRIAC-1">
<pin name="A2" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="M10">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="IQS133">
<pin name="GND"/>
<pin name="CX0"/>
<pin name="CX1"/>
<pin name="VDD"/>
<pin name="VR"/>
<pin name="TO2"/>
<pin name="CX2"/>
<pin name="TO1"/>
<pin name="TO0"/>
<pin name="P0"/>
</symbol>
<symbol name="CURRENTPLANK_STCS2A_STCS2A">
<pin name="DISC" direction="out"/>
<pin name="DRAIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="PWM" direction="in"/>
<pin name="SLOPE" direction="pas"/>
<pin name="SOURCE" direction="out"/>
<pin name="TAB" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="PIR">
<pin name="SOURCE" direction="out"/>
<pin name="GND" direction="sup"/>
<pin name="DRAIN" direction="pas"/>
</symbol>
<symbol name="LED-THERMAL">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="T" direction="nc"/>
</symbol>
<symbol name="PEG">
</symbol>
<symbol name="SPARK_LOGO">
</symbol>
<symbol name="SPARK_LOGO2">
</symbol>
<symbol name="SPARK_CORE">
<pin name="VIN" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="A0"/>
<pin name="3V3" direction="pwr"/>
<pin name="!RST"/>
<pin name="3V3*" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="D0"/>
</symbol>
<symbol name="SRD-5VDC-SL-C">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
</symbol>
<symbol name="RELAY-SPDT">
<pin name="COIL2"/>
<pin name="MAIN"/>
<pin name="NO"/>
<pin name="NC"/>
<pin name="COIL1"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
<symbol name="Q">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="SST25VF040B">
<pin name="VDD" direction="pwr"/>
<pin name="SI" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="WP" direction="in"/>
<pin name="HOLD" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="SO" direction="out"/>
</symbol>
<symbol name="VREG">
<pin name="IN" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="BNC-F2">
<pin name="1" direction="pas"/>
<pin name="GND@1" direction="pas"/>
</symbol>
<symbol name="ANTENNA">
<pin name="SIGNAL"/>
</symbol>
<symbol name="CAP_POL">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="SWITCH-MOMENTARY">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="M12">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="DIODE">
<pin name="ANODE"/>
<pin name="CATHODE"/>
</symbol>
<symbol name="POWERJACK">
<pin name="GNDBREAK"/>
<pin name="GND"/>
<pin name="PWR"/>
</symbol>
<symbol name="OSHW-LOGO">
</symbol>
<symbol name="NL17SZ125">
<pin name="/OE"/>
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT"/>
<pin name="VCC"/>
</symbol>
<symbol name="INDUCTOR-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="LM2672">
<pin name="CB"/>
<pin name="SS"/>
<pin name="SYNC"/>
<pin name="FB"/>
<pin name="ON/!OFF"/>
<pin name="GND" direction="pwr"/>
<pin name="VIN" direction="pwr"/>
<pin name="VSW"/>
</symbol>
<symbol name="AP1509-50SG-13">
<pin name="VIN"/>
<pin name="VOUT"/>
<pin name="FB"/>
<pin name="SD"/>
<pin name="GND5"/>
<pin name="GND6"/>
<pin name="GND7"/>
<pin name="GND8"/>
</symbol>
<symbol name="DHT22">
<pin name="VDD" direction="pwr"/>
<pin name="DATA" direction="out"/>
<pin name="NULL" direction="nc"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="TGS2602">
<pin name="H+"/>
<pin name="H-"/>
<pin name="S+"/>
<pin name="S-"/>
</symbol>
<symbol name="MICS5525">
<pin name="H+"/>
<pin name="H-"/>
<pin name="S-"/>
<pin name="S+"/>
</symbol>
<symbol name="MQ_SENSOR_SOCKET">
<pin name="A1"/>
<pin name="A2"/>
<pin name="H+"/>
<pin name="H-"/>
<pin name="B2"/>
<pin name="B1"/>
</symbol>
<symbol name="TESTPAD">
<pin name="TP"/>
</symbol>
<symbol name="NC74SZ11">
<pin name="1" direction="in"/>
<pin name="3" direction="in"/>
<pin name="6" direction="in"/>
<pin name="4" direction="out"/>
<pin name="2"/>
<pin name="5"/>
</symbol>
<symbol name="WM-N-BM-09">
<pin name="GPIO_7"/>
<pin name="GPIO_6"/>
<pin name="GPIO_5"/>
<pin name="GPIO_4"/>
<pin name="GPIO_3"/>
<pin name="GPIO_2"/>
<pin name="GPIO_1"/>
<pin name="GPIO_0"/>
<pin name="BTCX_RF_ACTIVE"/>
<pin name="BTCX_STATUS"/>
<pin name="BTCX_TXCONF"/>
<pin name="RF_SW_CTRL3_ANT1"/>
<pin name="RF_SW_CTRL0_ANT0"/>
<pin name="GND@14"/>
<pin name="ANT"/>
<pin name="GND@16"/>
<pin name="GND@17"/>
<pin name="GND@18"/>
<pin name="VDD_WIFI@19"/>
<pin name="VDD_WIFI@20"/>
<pin name="GND@21"/>
<pin name="SPI_SS"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_SCK"/>
<pin name="SPI_MISO"/>
<pin name="!MCU_RST"/>
<pin name="MCU_WKUP"/>
<pin name="VBAT"/>
<pin name="GND@29"/>
<pin name="GND@30"/>
<pin name="NC@31"/>
<pin name="NC@32"/>
<pin name="NC@33"/>
<pin name="NC@34"/>
<pin name="NC@35"/>
<pin name="NC@36"/>
<pin name="GND@37"/>
<pin name="MCU_UART_RX"/>
<pin name="MCU_UART_TX"/>
<pin name="JTAG_TCK"/>
<pin name="JTAG_TDO"/>
<pin name="!JTAG_TRST"/>
<pin name="JTAG_TDI"/>
<pin name="JTAG_TMS"/>
<pin name="GND@45"/>
<pin name="VDD_3V3@46"/>
<pin name="VDD_3V3@47"/>
<pin name="GND@48"/>
<pin name="VDDIO_WIFI"/>
<pin name="GND@50"/>
<pin name="MCU_USB_DP"/>
<pin name="MCU_USB_DN"/>
<pin name="GPIO_9"/>
<pin name="GPIO_8"/>
<pin name="GND@55"/>
<pin name="GND@56"/>
<pin name="GND@57"/>
<pin name="GND@58"/>
<pin name="GND@59"/>
<pin name="GND@60"/>
<pin name="GND@61"/>
<pin name="GND@62"/>
<pin name="GND@63"/>
<pin name="GND@64"/>
<pin name="GND@65"/>
<pin name="GND@66"/>
<pin name="GND@67"/>
</symbol>
<symbol name="AT45DB161E">
<pin name="SI"/>
<pin name="SCK"/>
<pin name="!RST"/>
<pin name="!CS"/>
<pin name="!WP"/>
<pin name="VCC"/>
<pin name="GND"/>
<pin name="SO"/>
</symbol>
<symbol name="20P">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="20" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="UCC28700">
<gates>
<gate name="G$1" symbol="UCC28700"/>
</gates>
<devices>
<device name="A" package="DBV">
<connects>
<connect gate="G$1" pin="CBC" pad="1"/>
<connect gate="G$1" pin="CS" pad="4"/>
<connect gate="G$1" pin="DRV" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOPLED-3" prefix="LED" uservalue="yes">
<description>&lt;b&gt;Cree&lt;/b&gt;&lt;p&gt;
CLVBA-FKA</description>
<gates>
<gate name="G$1" symbol="LED-RGB"/>
</gates>
<devices>
<device name="P-LCC-4" package="P-LCC-4">
<connects>
<connect gate="G$1" pin="A2" pad="A"/>
<connect gate="G$1" pin="CBLUE" pad="C@3"/>
<connect gate="G$1" pin="CGREEN" pad="C@4"/>
<connect gate="G$1" pin="CRED" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PLCC" package="P-LCC-4-3">
<connects>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="CBLUE" pad="3"/>
<connect gate="G$1" pin="CGREEN" pad="4"/>
<connect gate="G$1" pin="CRED" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CREE_CLVBA-FKA" package="P-LCC-4-3">
<connects>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="CBLUE" pad="1"/>
<connect gate="G$1" pin="CGREEN" pad="2"/>
<connect gate="G$1" pin="CRED" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EMC13" prefix="TR" uservalue="yes">
<description>&lt;b&gt;TRANSFORMER&lt;/b&gt;&lt;p&gt;
SMD toroidal-core transformer with 3 windings</description>
<gates>
<gate name="G$1" symbol="SMR6-3"/>
</gates>
<devices>
<device name="" package="EMC13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR">
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="A" package="B82464">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BT136" prefix="T">
<description>&lt;b&gt;Triac BT136 series E sensitive gate&lt;/b&gt;&lt;p&gt;
Source: http://www.nxp.com/acrobat_download/datasheets/BT136_SERIES_E_2.pdf</description>
<gates>
<gate name="-1" symbol="TRIAC-1"/>
</gates>
<devices>
<device name="" package="TO220AB">
<connects>
<connect gate="-1" pin="A1" pad="1"/>
<connect gate="-1" pin="A2" pad="2"/>
<connect gate="-1" pin="G" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="T435-TRIAC">
<gates>
<gate name="G$1" symbol="TRIAC-1"/>
</gates>
<devices>
<device name="DPAK" package="TO252">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="G" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M10" prefix="JP">
<description>&lt;b&gt;Header 10&lt;/b&gt;
Standard 10-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M10"/>
</gates>
<devices>
<device name="&quot;" package="1X10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MM" package="1X10-2MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2MMSMD" package="1X10-2MM-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X10_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X10_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MALE-SMD" package="1X10-2MM-MALE-SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IQS133">
<gates>
<gate name="G$1" symbol="IQS133"/>
</gates>
<devices>
<device name="IQS133" package="MSOP10">
<connects>
<connect gate="G$1" pin="CX0" pad="2"/>
<connect gate="G$1" pin="CX1" pad="3"/>
<connect gate="G$1" pin="CX2" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="P0" pad="10"/>
<connect gate="G$1" pin="TO0" pad="9"/>
<connect gate="G$1" pin="TO1" pad="8"/>
<connect gate="G$1" pin="TO2" pad="6"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VR" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CURRENTPLANK_STCS2A_STCS2A" prefix="IC" uservalue="yes">
<description>2 A max constant current LED driver</description>
<gates>
<gate name="G$1" symbol="CURRENTPLANK_STCS2A_STCS2A"/>
</gates>
<devices>
<device name="" package="CURRENTPLANK_STCS2A_POWER-SO10">
<connects>
<connect gate="G$1" pin="DISC" pad="10"/>
<connect gate="G$1" pin="DRAIN" pad="5"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="7"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="PWM" pad="2"/>
<connect gate="G$1" pin="SLOPE" pad="9"/>
<connect gate="G$1" pin="SOURCE" pad="6"/>
<connect gate="G$1" pin="TAB" pad="P"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XLAMP-XPE" prefix="LED">
<description>&lt;b&gt;Cree® XLamp® XP-E LEDs&lt;/b&gt;&lt;p&gt;
Source: www.cree.com/xlamp .. XLampXP-E.pdf</description>
<gates>
<gate name="LED$1" symbol="LED"/>
</gates>
<devices>
<device name="XLAMP" package="CREE_XLAMP">
<connects>
<connect gate="LED$1" pin="A" pad="A A@1"/>
<connect gate="LED$1" pin="C" pad="C C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIR_RE200B">
<description>&lt;B&gt;PIR&lt;/B&gt; - RE200</description>
<gates>
<gate name="PIR" symbol="PIR"/>
</gates>
<devices>
<device name="" package="RE200B">
<connects>
<connect gate="PIR" pin="DRAIN" pad="DRAIN+"/>
<connect gate="PIR" pin="GND" pad="GND"/>
<connect gate="PIR" pin="SOURCE" pad="SOURCE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XLAMP-XPE-THERMAL">
<gates>
<gate name="LED$1" symbol="LED-THERMAL"/>
</gates>
<devices>
<device name="" package="CREE_XLAMP">
<connects>
<connect gate="LED$1" pin="A" pad="A A@1"/>
<connect gate="LED$1" pin="C" pad="C C@1"/>
<connect gate="LED$1" pin="T" pad="X"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARK_LOGO">
<gates>
<gate name="G$1" symbol="SPARK_LOGO"/>
</gates>
<devices>
<device name=".." package="SPARK_LOGO">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SPARK_LOGO_TSTOP">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARK_LOGO2">
<gates>
<gate name="G$1" symbol="SPARK_LOGO"/>
</gates>
<devices>
<device name="" package="SPARK_LOGO2">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARK_CORE">
<gates>
<gate name="G$1" symbol="SPARK_CORE"/>
</gates>
<devices>
<device name="CORE" package="SPARK_CORE">
<connects>
<connect gate="G$1" pin="!RST" pad="23"/>
<connect gate="G$1" pin="3V3" pad="24"/>
<connect gate="G$1" pin="3V3*" pad="22"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="17"/>
<connect gate="G$1" pin="D5" pad="18"/>
<connect gate="G$1" pin="D6" pad="19"/>
<connect gate="G$1" pin="D7" pad="20"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@21" pad="21"/>
<connect gate="G$1" pin="RX" pad="4"/>
<connect gate="G$1" pin="TX" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SPARK_CORE_STACKABLE">
<connects>
<connect gate="G$1" pin="!RST" pad="#23 23 @23"/>
<connect gate="G$1" pin="3V3" pad="#24 24 @24"/>
<connect gate="G$1" pin="3V3*" pad="#22 22 @22"/>
<connect gate="G$1" pin="A0" pad="#12 12 @12"/>
<connect gate="G$1" pin="A1" pad="#11 11 @11"/>
<connect gate="G$1" pin="A2" pad="#10 10 @10"/>
<connect gate="G$1" pin="A3" pad="#9 9 @9"/>
<connect gate="G$1" pin="A4" pad="#8 8 @8"/>
<connect gate="G$1" pin="A5" pad="#7 7 @7"/>
<connect gate="G$1" pin="A6" pad="#6 6 @6"/>
<connect gate="G$1" pin="A7" pad="#5 5 @5"/>
<connect gate="G$1" pin="D0" pad="#13 13 @13"/>
<connect gate="G$1" pin="D1" pad="#14 14 @14"/>
<connect gate="G$1" pin="D2" pad="#15 15 @15"/>
<connect gate="G$1" pin="D3" pad="#16 16 @16"/>
<connect gate="G$1" pin="D4" pad="#17 17 @17"/>
<connect gate="G$1" pin="D5" pad="#18 18 @18"/>
<connect gate="G$1" pin="D6" pad="#19 19 @19"/>
<connect gate="G$1" pin="D7" pad="#20 20 @20"/>
<connect gate="G$1" pin="GND@2" pad="#2 2 @2"/>
<connect gate="G$1" pin="GND@21" pad="#21 21 @21"/>
<connect gate="G$1" pin="RX" pad="#4 4 @4"/>
<connect gate="G$1" pin="TX" pad="#3 3 @3"/>
<connect gate="G$1" pin="VIN" pad="#1 1 @1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARK_LOGO_WITH_PLANE">
<gates>
<gate name="G$1" symbol="SPARK_LOGO"/>
</gates>
<devices>
<device name="" package="SPARK_LOGO_PLUS_PLANE">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RELAY">
<description>SPDT relay (COM-00101)</description>
<gates>
<gate name="G$1" symbol="RELAY-SPDT"/>
</gates>
<devices>
<device name="PTH" package="RELAY-G5Q">
<connects>
<connect gate="G$1" pin="COIL1" pad="5"/>
<connect gate="G$1" pin="COIL2" pad="1"/>
<connect gate="G$1" pin="MAIN" pad="2"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="NO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="RELAY-T9A">
<connects>
<connect gate="G$1" pin="COIL1" pad="COIL1"/>
<connect gate="G$1" pin="COIL2" pad="COIL2"/>
<connect gate="G$1" pin="MAIN" pad="MAIN"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH3" package="RELAY-T9A-2">
<connects>
<connect gate="G$1" pin="COIL1" pad="COIL1"/>
<connect gate="G$1" pin="COIL2" pad="COIL2"/>
<connect gate="G$1" pin="MAIN" pad="MAIN"/>
<connect gate="G$1" pin="NC" pad="NC"/>
<connect gate="G$1" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH4" package="RELAY-JZC">
<connects>
<connect gate="G$1" pin="COIL1" pad="5"/>
<connect gate="G$1" pin="COIL2" pad="1"/>
<connect gate="G$1" pin="MAIN" pad="4"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SONGLE" package="SRD-5VDC-SL-C">
<connects>
<connect gate="G$1" pin="COIL1" pad="COIL1"/>
<connect gate="G$1" pin="COIL2" pad="COIL2"/>
<connect gate="G$1" pin="MAIN" pad="COMMON"/>
<connect gate="G$1" pin="NC" pad="CLOSED"/>
<connect gate="G$1" pin="NO" pad="OPEN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PANASONIC-JS" package="JS1-5V-F">
<connects>
<connect gate="G$1" pin="COIL1" pad="COIL1"/>
<connect gate="G$1" pin="COIL2" pad="COIL2"/>
<connect gate="G$1" pin="MAIN" pad="COMMON"/>
<connect gate="G$1" pin="NC" pad="CLOSED"/>
<connect gate="G$1" pin="NO" pad="OPEN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OMRON" package="G5LE-14-DC5">
<connects>
<connect gate="G$1" pin="COIL1" pad="COIL1"/>
<connect gate="G$1" pin="COIL2" pad="COIL2"/>
<connect gate="G$1" pin="MAIN" pad="COMMON"/>
<connect gate="G$1" pin="NC" pad="CLOSED"/>
<connect gate="G$1" pin="NO" pad="OPEN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB" prefix="JP">
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="-A-H" package="USB-A-H">
<connects>
<connect gate="G$1" pin="D+" pad="D-"/>
<connect gate="G$1" pin="D-" pad="D+"/>
<connect gate="G$1" pin="GND" pad="VBUS"/>
<connect gate="G$1" pin="VBUS" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-S" package="USB-A-S">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MB-H" package="USB-MB-H">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B-S" package="USB-B-SMT">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VUSB"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OLD" package="USB-MINIB-OLD">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="USB-B-PTH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08278"/>
<attribute name="VALUE" value="USB-B"/>
</technology>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="S4B-PH">
<connects>
<connect gate="G$1" pin="D+" pad="2"/>
<connect gate="G$1" pin="D-" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VBUS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="USB-MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PCB" package="USB-A-PCB">
<connects>
<connect gate="G$1" pin="D+" pad="USB_P"/>
<connect gate="G$1" pin="D-" pad="USB_M"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="5V"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-VERTICAL" package="USB-B-PTH-VERTICAL">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="USB-A-S-NOSILK" package="USB-A-S-NOSILK">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-A-SMD" package="USB-A-S-NOSILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09520"/>
</technology>
</technologies>
</device>
<device name="-SMD-NS" package="USB-MINIB-NOSTOP">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="USB-A-S-SILK-FEMALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MICROB" package="USB-MICROB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND MT1 MT2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-09505"/>
</technology>
</technologies>
</device>
<device name="A-SMD-MALE" package="USB-A-SMT-MALE">
<connects>
<connect gate="G$1" pin="D+" pad="D+1"/>
<connect gate="G$1" pin="D-" pad="D-1"/>
<connect gate="G$1" pin="GND" pad="GND1"/>
<connect gate="G$1" pin="VBUS" pad="VBUS1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="USB-MICROB-ALIGN" package="USB-MICROB-ALIGN">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND MT1 MT2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="USB-MICROB-SMT-DIP" package="USB-MICROB-SMT-DIP">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND MT1 MT2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="USB-MICROB-SLOT-HOLE" package="USB-MICROB-SLOT-HOLE">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND MT1 MT2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FCI" package="USB-MICROB-MALE-SANDWICH">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND GNDPAD1 GNDPAD2"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="Q" prefix="Q" uservalue="yes">
<gates>
<gate name="G$1" symbol="Q"/>
</gates>
<devices>
<device name="_FC135" package="FC135">
<connects>
<connect gate="G$1" pin="1" pad="X1"/>
<connect gate="G$1" pin="2" pad="X2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_HC49UP" package="HC49UP">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TC38" package="TC38">
<connects>
<connect gate="G$1" pin="1" pad="+"/>
<connect gate="G$1" pin="2" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49U-H" package="HC49U-H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49U-V" package="HC49U-V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_TC38-SMD" package="TC38-SMD">
<connects>
<connect gate="G$1" pin="1" pad="X1"/>
<connect gate="G$1" pin="2" pad="X2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_3.2X2.5" package="OSC3.2X.2.5">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SST25VF040B" prefix="U">
<description>4 Mbit SPI Serial Flash</description>
<gates>
<gate name="A" symbol="SST25VF040B"/>
</gates>
<devices>
<device name="-S2" package="SOIC127P790X216-8N">
<connects>
<connect gate="A" pin="CE" pad="1"/>
<connect gate="A" pin="HOLD" pad="7"/>
<connect gate="A" pin="SCK" pad="6"/>
<connect gate="A" pin="SI" pad="5"/>
<connect gate="A" pin="SO" pad="2"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VSS" pad="4"/>
<connect gate="A" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-Q" package="WSON-8-PAD">
<connects>
<connect gate="A" pin="CE" pad="1"/>
<connect gate="A" pin="HOLD" pad="7"/>
<connect gate="A" pin="SCK" pad="6"/>
<connect gate="A" pin="SI" pad="5"/>
<connect gate="A" pin="SO" pad="2"/>
<connect gate="A" pin="VDD" pad="8"/>
<connect gate="A" pin="VSS" pad="4"/>
<connect gate="A" pin="WP" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1825S" prefix="IC" uservalue="yes">
<description>500 mA, Low Voltage, Low Quiescent Current LDO Regulator</description>
<gates>
<gate name="G$1" symbol="VREG"/>
</gates>
<devices>
<device name="-SOT223" package="SOT223">
<connects>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IPEX-20279-001E" prefix="X">
<description>Ultra Miniature Coaxial SMT RF Receptacle</description>
<gates>
<gate name="G$1" symbol="BNC-F2"/>
</gates>
<devices>
<device name="" package="IPEX-20279-001E">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2@1 2@2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT8010" prefix="ANT">
<description>AT8010 Series Multilayer Chip Antenna</description>
<gates>
<gate name="G$1" symbol="ANTENNA"/>
</gates>
<devices>
<device name="" package="AT8010">
<connects>
<connect gate="G$1" pin="SIGNAL" pad="SIG"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TANT-CAP" prefix="C" uservalue="yes">
<description>Tantalum SMT</description>
<gates>
<gate name="G$1" symbol="CAP_POL"/>
</gates>
<devices>
<device name="1206" package="EIA3216">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="PC0603">
<connects>
<connect gate="G$1" pin="+" pad="A"/>
<connect gate="G$1" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TAC_SWITCH" prefix="S" uservalue="yes">
<description>SMD Tactiile Switch</description>
<gates>
<gate name="S" symbol="SWITCH-MOMENTARY"/>
</gates>
<devices>
<device name="SMD" package="TACTILE_SWITCH_SMD">
<connects>
<connect gate="S" pin="1" pad="1"/>
<connect gate="S" pin="2" pad="2"/>
<connect gate="S" pin="3" pad="3"/>
<connect gate="S" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M12" prefix="JP">
<description>&lt;b&gt;Header 12&lt;/b&gt;
Standard 12-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115).</description>
<gates>
<gate name="G$1" symbol="M12"/>
</gates>
<devices>
<device name="PTH" package="1X12-SMALL-PADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE">
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="DIODE-DO-220AA(SMP)">
<connects>
<connect gate="G$1" pin="ANODE" pad="ANODE"/>
<connect gate="G$1" pin="CATHODE" pad="CATHODE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POWER_JACK" prefix="J">
<description>&lt;b&gt;Power Jack&lt;/b&gt;
This is the standard 5.5mm barrel jack for power.&lt;br&gt;
The PTH is the most common, proven, reliable, footprint.&lt;br&gt;
The Slot footprint only works if the mill layer is transmitted to the PCB fab house so be warned.&lt;br&gt;
Spark Fun Electronics SKU : PRT-00119&lt;br&gt;
SMT: CONN-08106&lt;br&gt;

Mating wall wart : TOL-00298 (and others)</description>
<gates>
<gate name="G$1" symbol="POWERJACK"/>
</gates>
<devices>
<device name="SMD" package="POWER_JACK_SMD">
<connects>
<connect gate="G$1" pin="GND" pad="P$4"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="VIN0"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="CONN-08106"/>
<attribute name="VALUE" value="5.5x2.1mm Barrel"/>
</technology>
</technologies>
</device>
<device name="SLT" package="POWER_JACK_SLOT">
<connects>
<connect gate="G$1" pin="GND" pad="GND@2"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND@1"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH" package="POWER_JACK_PTH">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="COMBO" package="POWER_JACK_COMBO">
<connects>
<connect gate="G$1" pin="GND" pad="GND@1"/>
<connect gate="G$1" pin="GNDBREAK" pad="GND"/>
<connect gate="G$1" pin="PWR" pad="POWER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_LOCK" package="POWER_JACK_PTH_LOCK">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="GNDBREAK" pad="GNDBREAK"/>
<connect gate="G$1" pin="PWR" pad="PWR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSHW-LOGO" prefix="LOGO">
<description>&lt;b&gt;Open Source Hardware Logo&lt;/b&gt; This logo indicates the piece of hardware it is found on incorporates a OSHW license and/or adheres to the definition of open source hardware found here: http://freedomdefined.org/OSHW</description>
<gates>
<gate name="G$1" symbol="OSHW-LOGO"/>
</gates>
<devices>
<device name="S" package="OSHW-LOGO-S">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="OSHW-LOGO-M">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L" package="OSHW-LOGO-L">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL17SZ125">
<gates>
<gate name="G$1" symbol="NL17SZ125"/>
</gates>
<devices>
<device name="SOT553" package="SOT-553">
<connects>
<connect gate="G$1" pin="/OE" pad="/OE"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT953" package="SOT-953">
<connects>
<connect gate="G$1" pin="/OE" pad="/OE"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR-SPARKFUN" prefix="L" uservalue="yes">
<description>&lt;b&gt;Inductors&lt;/b&gt;&lt;p&gt;
Basic Inductor/Choke - 0603 and 1206. Footprints are not proven and vary greatly between part numbers.&lt;br&gt;
SRN6045- 33uH, 20% 1.4A</description>
<gates>
<gate name="G$1" symbol="INDUCTOR-1"/>
</gates>
<devices>
<device name="H*" package="INDUCTOR-1206">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="1206"/>
</technologies>
</device>
<device name="0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR54" package="CR54">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PWR" package="CDRH125">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B82462G" package="B82462G">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR75" package="CR75">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1007" package="1007">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_" package="COOPER_UP4B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-" package="CDRH3D28">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR75_V2" package="CR75_V2">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="." package="CDRH2D09">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NPI75" package="NPI75C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SRU5028" package="SRU5028">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SRU1038" package="SRU1038">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR54-KIT" package="CR54-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DR1030" package="DR1030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VLF4012A" package="VLF4012A">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AXIAL-0.6" package="AXIAL-0.6">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RLB0912" package="RLB0912">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BOURNS_SRN6045" package="SRN6045">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="NDUC-11627"/>
<attribute name="VALUE" value="33uH"/>
</technology>
</technologies>
</device>
<device name="NR3015T4R7M" package="INDUCTOR-NR3015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="NR3015T4R7M" value="4.7uH"/>
</technology>
</technologies>
</device>
<device name="VLS3012ET-4R7M" package="INDUCTOR-VLS-E">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="INDUCTOR-SDR1005-470KL">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2672">
<gates>
<gate name="G$1" symbol="LM2672"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="CB" pad="1"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="ON/!OFF" pad="5"/>
<connect gate="G$1" pin="SS" pad="2"/>
<connect gate="G$1" pin="SYNC" pad="3"/>
<connect gate="G$1" pin="VIN" pad="7"/>
<connect gate="G$1" pin="VSW" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AP1509-50SG-13">
<gates>
<gate name="G$1" symbol="AP1509-50SG-13"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND5" pad="5"/>
<connect gate="G$1" pin="GND6" pad="6"/>
<connect gate="G$1" pin="GND7" pad="7"/>
<connect gate="G$1" pin="GND8" pad="8"/>
<connect gate="G$1" pin="SD" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DHT22">
<gates>
<gate name="G$1" symbol="DHT22"/>
</gates>
<devices>
<device name="" package="DHT22">
<connects>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="NULL" pad="NC"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TGS2602">
<gates>
<gate name="G$1" symbol="TGS2602"/>
</gates>
<devices>
<device name="" package="TGS2602">
<connects>
<connect gate="G$1" pin="H+" pad="HEATER+"/>
<connect gate="G$1" pin="H-" pad="HEATER-"/>
<connect gate="G$1" pin="S+" pad="SENSOR+"/>
<connect gate="G$1" pin="S-" pad="SENSOR-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICS5525">
<gates>
<gate name="G$1" symbol="MICS5525"/>
</gates>
<devices>
<device name="" package="MICS5525">
<connects>
<connect gate="G$1" pin="H+" pad="H+"/>
<connect gate="G$1" pin="H-" pad="H-"/>
<connect gate="G$1" pin="S+" pad="S+"/>
<connect gate="G$1" pin="S-" pad="S-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MQ_SENSOR_SOCKET">
<gates>
<gate name="G$1" symbol="MQ_SENSOR_SOCKET"/>
</gates>
<devices>
<device name="" package="MQ_SENSOR_SOCKET">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="7"/>
<connect gate="G$1" pin="B1" pad="3"/>
<connect gate="G$1" pin="B2" pad="1"/>
<connect gate="G$1" pin="H+" pad="6"/>
<connect gate="G$1" pin="H-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TESTPAD-PTR">
<gates>
<gate name="G$1" symbol="TESTPAD"/>
</gates>
<devices>
<device name="" package="TESTPAD-PTR">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NC7SZ11" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="NC74SZ11"/>
</gates>
<devices>
<device name="" package="SC70-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WM-N-BM-09" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="WM-N-BM-09"/>
</gates>
<devices>
<device name="" package="WM-N-BM-09">
<connects>
<connect gate="G$1" pin="!JTAG_TRST" pad="P$42"/>
<connect gate="G$1" pin="!MCU_RST" pad="P$26"/>
<connect gate="G$1" pin="ANT" pad="P$15"/>
<connect gate="G$1" pin="BTCX_RF_ACTIVE" pad="P$9"/>
<connect gate="G$1" pin="BTCX_STATUS" pad="P$10"/>
<connect gate="G$1" pin="BTCX_TXCONF" pad="P$11"/>
<connect gate="G$1" pin="GND@14" pad="P$14"/>
<connect gate="G$1" pin="GND@16" pad="P$16"/>
<connect gate="G$1" pin="GND@17" pad="P$17"/>
<connect gate="G$1" pin="GND@18" pad="P$18"/>
<connect gate="G$1" pin="GND@21" pad="P$21"/>
<connect gate="G$1" pin="GND@29" pad="P$29"/>
<connect gate="G$1" pin="GND@30" pad="P$30"/>
<connect gate="G$1" pin="GND@37" pad="P$37"/>
<connect gate="G$1" pin="GND@45" pad="P$45"/>
<connect gate="G$1" pin="GND@48" pad="P$48"/>
<connect gate="G$1" pin="GND@50" pad="P$50"/>
<connect gate="G$1" pin="GND@55" pad="P$55"/>
<connect gate="G$1" pin="GND@56" pad="P$56"/>
<connect gate="G$1" pin="GND@57" pad="P$57"/>
<connect gate="G$1" pin="GND@58" pad="P$58"/>
<connect gate="G$1" pin="GND@59" pad="P$59"/>
<connect gate="G$1" pin="GND@60" pad="P$60"/>
<connect gate="G$1" pin="GND@61" pad="P$61"/>
<connect gate="G$1" pin="GND@62" pad="P$62"/>
<connect gate="G$1" pin="GND@63" pad="P$63"/>
<connect gate="G$1" pin="GND@64" pad="P$64"/>
<connect gate="G$1" pin="GND@65" pad="P$65"/>
<connect gate="G$1" pin="GND@66" pad="P$66"/>
<connect gate="G$1" pin="GND@67" pad="P$67"/>
<connect gate="G$1" pin="GPIO_0" pad="P$8"/>
<connect gate="G$1" pin="GPIO_1" pad="P$7"/>
<connect gate="G$1" pin="GPIO_2" pad="P$6"/>
<connect gate="G$1" pin="GPIO_3" pad="P$5"/>
<connect gate="G$1" pin="GPIO_4" pad="P$4"/>
<connect gate="G$1" pin="GPIO_5" pad="P$3"/>
<connect gate="G$1" pin="GPIO_6" pad="P$2"/>
<connect gate="G$1" pin="GPIO_7" pad="P$1"/>
<connect gate="G$1" pin="GPIO_8" pad="P$54"/>
<connect gate="G$1" pin="GPIO_9" pad="P$53"/>
<connect gate="G$1" pin="JTAG_TCK" pad="P$40"/>
<connect gate="G$1" pin="JTAG_TDI" pad="P$43"/>
<connect gate="G$1" pin="JTAG_TDO" pad="P$41"/>
<connect gate="G$1" pin="JTAG_TMS" pad="P$44"/>
<connect gate="G$1" pin="MCU_UART_RX" pad="P$38"/>
<connect gate="G$1" pin="MCU_UART_TX" pad="P$39"/>
<connect gate="G$1" pin="MCU_USB_DN" pad="P$52"/>
<connect gate="G$1" pin="MCU_USB_DP" pad="P$51"/>
<connect gate="G$1" pin="MCU_WKUP" pad="P$27"/>
<connect gate="G$1" pin="NC@31" pad="P$31"/>
<connect gate="G$1" pin="NC@32" pad="P$32"/>
<connect gate="G$1" pin="NC@33" pad="P$33"/>
<connect gate="G$1" pin="NC@34" pad="P$34"/>
<connect gate="G$1" pin="NC@35" pad="P$35"/>
<connect gate="G$1" pin="NC@36" pad="P$36"/>
<connect gate="G$1" pin="RF_SW_CTRL0_ANT0" pad="P$13"/>
<connect gate="G$1" pin="RF_SW_CTRL3_ANT1" pad="P$12"/>
<connect gate="G$1" pin="SPI_MISO" pad="P$25"/>
<connect gate="G$1" pin="SPI_MOSI" pad="P$23"/>
<connect gate="G$1" pin="SPI_SCK" pad="P$24"/>
<connect gate="G$1" pin="SPI_SS" pad="P$22"/>
<connect gate="G$1" pin="VBAT" pad="P$28"/>
<connect gate="G$1" pin="VDDIO_WIFI" pad="P$49"/>
<connect gate="G$1" pin="VDD_3V3@46" pad="P$46"/>
<connect gate="G$1" pin="VDD_3V3@47" pad="P$47"/>
<connect gate="G$1" pin="VDD_WIFI@19" pad="P$19"/>
<connect gate="G$1" pin="VDD_WIFI@20" pad="P$20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB161E" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="AT45DB161E"/>
</gates>
<devices>
<device name="SOIC8" package="SO08">
<connects>
<connect gate="G$1" pin="!CS" pad="4"/>
<connect gate="G$1" pin="!RST" pad="3"/>
<connect gate="G$1" pin="!WP" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ML20" prefix="SV" uservalue="yes">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="20P"/>
</gates>
<devices>
<device name="" package="ML20">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="10" pad="10"/>
<connect gate="1" pin="11" pad="11"/>
<connect gate="1" pin="12" pad="12"/>
<connect gate="1" pin="13" pad="13"/>
<connect gate="1" pin="14" pad="14"/>
<connect gate="1" pin="15" pad="15"/>
<connect gate="1" pin="16" pad="16"/>
<connect gate="1" pin="17" pad="17"/>
<connect gate="1" pin="18" pad="18"/>
<connect gate="1" pin="19" pad="19"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="20" pad="20"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="1" pin="6" pad="6"/>
<connect gate="1" pin="7" pad="7"/>
<connect gate="1" pin="8" pad="8"/>
<connect gate="1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L" package="ML20L">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="10" pad="10"/>
<connect gate="1" pin="11" pad="11"/>
<connect gate="1" pin="12" pad="12"/>
<connect gate="1" pin="13" pad="13"/>
<connect gate="1" pin="14" pad="14"/>
<connect gate="1" pin="15" pad="15"/>
<connect gate="1" pin="16" pad="16"/>
<connect gate="1" pin="17" pad="17"/>
<connect gate="1" pin="18" pad="18"/>
<connect gate="1" pin="19" pad="19"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="20" pad="20"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="1" pin="6" pad="6"/>
<connect gate="1" pin="7" pad="7"/>
<connect gate="1" pin="8" pad="8"/>
<connect gate="1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="3M" package="3M_20">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="10" pad="10"/>
<connect gate="1" pin="11" pad="11"/>
<connect gate="1" pin="12" pad="12"/>
<connect gate="1" pin="13" pad="13"/>
<connect gate="1" pin="14" pad="14"/>
<connect gate="1" pin="15" pad="15"/>
<connect gate="1" pin="16" pad="16"/>
<connect gate="1" pin="17" pad="17"/>
<connect gate="1" pin="18" pad="18"/>
<connect gate="1" pin="19" pad="19"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="20" pad="20"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="1" pin="6" pad="6"/>
<connect gate="1" pin="7" pad="7"/>
<connect gate="1" pin="8" pad="8"/>
<connect gate="1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="3ML" package="3M_20L">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="10" pad="10"/>
<connect gate="1" pin="11" pad="11"/>
<connect gate="1" pin="12" pad="12"/>
<connect gate="1" pin="13" pad="13"/>
<connect gate="1" pin="14" pad="14"/>
<connect gate="1" pin="15" pad="15"/>
<connect gate="1" pin="16" pad="16"/>
<connect gate="1" pin="17" pad="17"/>
<connect gate="1" pin="18" pad="18"/>
<connect gate="1" pin="19" pad="19"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="20" pad="20"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="4" pad="4"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="1" pin="6" pad="6"/>
<connect gate="1" pin="7" pad="7"/>
<connect gate="1" pin="8" pad="8"/>
<connect gate="1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
